Is There Asbestos?   isthereasbestos.co.uk  ·  Asbestos management plan and register  ·  Free template v1.0, October 2026
Asbestos management plan and register
For dutyholders of non-domestic premises and common parts of domestic premises
	1. Premises and survey



	Premises name and address
	Dutyholder (organisation)

	 
	 

	Survey type (management / refurbishment and demolition)
	Surveyor and survey date

	 
	 

	Survey report reference
	Date of this plan

	 
	 



	2. Who is responsible



HSE says the plan should say who is responsible for managing asbestos, including deputies, and who is responsible for each part of the plan.
	Role
	Name
	Contact
	Responsible for

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	3. Site plan



	Where is the site plan showing ACMs and areas not inspected kept? (attach a copy)

	 



	4. Monitoring schedule



How often you will check the condition of each ACM, and who does it.
	ACM ref
	Location
	Check frequency
	Next check due
	Checked by

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



	5. Sharing the register



	How the register and plan are shared with workers and contractors before they work on the building fabric (e.g. shown at sign-in, sent with requests for quotes)

	 





	6. Asbestos register



All known and presumed ACMs, the type, amount and condition, the dates of the original and last inspection, the material and priority assessment, and the action decided.
	Ref
	Location
	Material / product
	Extent
	Condition and date last inspected
	Material score
	Priority score
	Action and due date
	Done (date)

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	



	Areas not inspected (presumed to contain asbestos until inspected)

	 





	7. Control arrangements



	How you make sure ACMs are not disturbed (e.g. permit-to-work for work on the building fabric, labelling, restricted access, briefing contractors)

	 



	8. Emergency procedures



	What happens if ACMs are disturbed by accident: who stops work and keeps people out of the area, who is contacted, how the area is assessed and cleaned up

	 

	Information given to the emergency services about the location and condition of known ACMs

	 



	9. Review log



HSE says to review the plan at least every 12 months, and whenever work affects ACMs, when staff with management responsibilities change, after ACMs are disturbed by accident, and after scheduled condition checks.
	Date
	Reason for review
	Changes made
	Reviewed by

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



Based on: HSE guidance: the duty to manage asbestos, make a register and assess the risk, and write your asbestos management plan. Free template, not an HSE form. It is only as reliable as the survey behind it: any area not inspected must be presumed to contain asbestos until it is. Contains public sector information licensed under the Open Government Licence v3.0. General guidance, not legal advice.




